### STM32F407VET6 Dev Board

STM32F407VET6 (LQFP100)
- CPU: 168MHz
- Flash: 512KB
- SRAM: 192KB

<a href="url"><img src="./images/stm32vet6_board.png" width="400"></a>  

### Projects

- [ESP8266_AT_CMD_VET6](workspace/ESP8266_AT_CMD_VET6/)
- [ESP8266_TCP_Client_VET6](workspace/ESP8266_TCP_Client_VET6/)


